Company Letterhead

**Shipper's Declaration for Section II Lithium Cells / Batteries**

**WARNING:**

Shipment Details：

# LITHIUM BATTERIES IDENTIFIED BY THE MANUFACTURER AS BEING DEFECTIVE FOR SAFET REASONS, OR THAT HAVE BEEN DAMAGED, MUST NOT BE SHIPPED BY AIR.

Master Air Waybill Number： Origin：

House Air Waybill Number： Destination:

Shipper's Information:

**Name:
Address:**

**Contact Number:**

Consignee's Information:

**Name:**

**Address:**

**Contact Number:**

Select the applicable battery type(s) and fill in the blanks.

|  |  |
| --- | --- |
| Battery Type [IMP Code] Piece | Net Weight per Package (kg) |
| **UN3480 / PI965 [ELI]**Lithium Ion Cell/Batteries Only | Cell / Battery ≦2.7Wh |  |  |
| Cell > 2.7 Wh but ≦ 20 Wh |  |  |
| Battery > 2.7 Wh but ≦ 100Wh |  |  |
| **UN3481 / PI966 [ELI]**Lithium Ion Cells / Batteries Packed with Equipment |  |  |
| **UN3481 / PI967 [ELI]**Lithium Ion Cells / Batteries Contained with Equipment |  |  |
| **UN3090 / PI968 [ELM]**Lithium Metal Cells / Batteries Only | Cell / Battery ≦0.3g lithium |  |  |
| Cell > 03.g but ≦ 1g lithium |  |  |
| Battery > 03.g but ≦ 2g lithium |  |  |
| **UN3091 / PI969 [ELM]**Lithium Metal Cells / Batteries Packed with Equipment |  |  |
| **UN3091 / PI970 [ELM]**Lithium Metal Cells / Batteries Contained in Equipment |  |  |

Lithium **ION** cells/batteries in compliance with Section II of PI . Lithium **METAL** cells/batteries in compliance with Section II of PI .

* This package must be handled with care. A flammability hazard exists if the package is damaged.
* Special Procedures must be followed in in the event the package is damaged, to include inspection and repacking if necessary.

Special Procedures:

a.

b.

c.

Telephone Number For Additional Information

Remarks: **Name :**

MSDS NO.

UN38.3 NO.

Company Stamp: Date:

